Home > Network > Technical Information for Advanced Users > Other Ways to Configure the IP Address > Configure the IP Address Using APIPA

### Configure the IP Address Using APIPA

Related Models:HL‑L2340DW / HL‑L2360DN / HL‑L2365DW

The Brother print server supports the Automatic Private IP Addressing (APIPA) protocol. With APIPA, DHCP clients automatically configure an IP address and subnet mask when a DHCP server is not available. The device selects its own IP address in the range 169.254.1.0 through 169.254.254.255. The subnet mask is automatically set to 255.255.0.0 and the gateway address is set to 0.0.0.0.

By default, the APIPA protocol is enabled. To disable the APIPA protocol, use the machine's control panel, BRAdmin applications, or Web Based Management.

Related Information
  - Other Ways to Configure the IP Address

Go to top of page