Home > Network > Technical Information for Advanced Users > Additional Network Settings from Windows® > Install Drivers Used for Printing for Infrastructure Mode When Using Vertical Pairing (Windows® 7 and Windows® 8)

### Install Drivers Used for Printing for Infrastructure Mode When Using Vertical Pairing (Windows® 7 and Windows® 8)

Related Models:HL‑L2340DW / HL‑L2365DW
Windows® Vertical Pairing is a technology that allows your Vertical Pairing-supported wireless machine to connect to your Infrastructure network using the PIN Method of WPS and the Web Services feature. It enables printer driver installation from the printer icon in the Add a device screen. If you are in Infrastructure mode, you can connect your machine to the wireless network, and then install the printer driver using this feature.

- Verify that the host computer and the Brother machine are on the same subnet, or that the router is correctly configured to pass data between the two devices.
- If you have disabled your machine's Web Services feature, you must re-enable it by selecting the Web Services check box and clicking Submit. The default setting of Web Services for the Brother machine is Enabled. You can change the Web Services setting using Web Based Management or BRAdmin Professional 3.
- Make sure your wireless LAN access point/router has the Windows® 7 or Windows® 8 compatibility logo. If you are not sure about the compatibility logo, contact your access point/router manufacturer.
- Make sure your computer has the Windows® 7 or Windows® 8 compatibility logo. If you are not sure about the compatibility logo, contact your computer manufacturer.
- If you are configuring your wireless network using an external wireless Network Interface Card (NIC), make sure the wireless NIC has the Windows® 7 or Windows® 8 compatibility logo. For more information, contact your wireless NIC manufacturer.
- To use a Windows® 7 or a Windows® 8 computer as a Registrar, you must register it to your network in advance. See the instructions supplied with your wireless LAN access point/router.

1. Turn on your machine.
2. Set your machine to WPS mode (PIN Method).
3. Do one of the following:
   - (Windows® 7)

     Click (Start)>Devices and Printers>Add a device.

   - (Windows® 8)

     Move your mouse to the lower right corner of your desktop. When the menu bar appears, click Settings>Control Panel>Hardware and Sound>Devices and Printers>Add a device.

4. Select your machine and type the PIN.
5. Select the infrastructure network to which you want to connect, and then click Next.
6. When your machine appears in the Devices and Printers dialog box, the wireless configuration and the printer driver installation are successfully completed.

Related Information
  - Additional Network Settings from Windows®
  - Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

Go to top of page