Home > Specifications > General Specifications

### General Specifications

Printer Type | Laser
Print Method | Electrophotographic Laser Printer
Memory Capacity | Standard | (HL-L2300D) 8 MB (HL-L2340DW/HL-L2360DN/HL-L2365DW) 32 MB
LCD (liquid crystal display) | (HL-L2340DW/HL-L2360DN/HL-L2365DW) 16 characters × 1 line
Power Source | 220 - 240 V AC 50/60 Hz
Power Consumption (Average) | Peak *1 | Approximately 1080 W
Printing *1 | (HL-L2300D/HL-L2340DW) Approximately 455 W at 25 °C (/HL-L2360DN/HL-L2365DW) Approximately 537 W at 25 °C
Printing (Quiet Mode)*1 | (HL-L2300D/HL-L2340DW) Approximately 318 W at 25 °C (HL-L2360DN/HL-L2365DW) Approximately 331 W at 25 °C
Ready *1 | Approximately 58 W at 25 °C
Sleep *1 | Approximately 5.4 W
Networked Standby*2*3 | (HL-L2300D) Approximately 0.4 W (HL-L2360DN) Approximately 0.5 W (HL-L2340DW/HL-L2365DW)

Approximately 1.7 W

Deep Sleep *1 | (HL-L2300D) Approximately 0.4 W (HL-L2340DW/HL-L2360DN/HL-L2365DW) Approximately 0.5 W
Power Off*1*4*5 | Approximately 0.06 W
Dimensions |
Weights (with supplies) | 6.9 kg

*1
Measured when the machine is connected to the USB interface.
*2
All wireless network ports activated and all wired network ports connected according to Regulation (EU) No 801/2013.
*3
To activate and deactivate the wireless function, see Related Information.
*4
Measured according to IEC 62301 Edition 2.0.
*5
Power consumption varies slightly depending on the usage environment.

Noise Level | Sound Pressure | Printing | (HL-L2300D/HL-L2340DW) LpAm = 49 dB (A) (HL-L2360DN/HL-L2365DW) LpAm = 50 dB (A)
Ready | LpAm = 30 dB (A)
Printing (Quiet Mode) | LpAm = 45 dB (A)
Sound Power | Printing *1*2 | (HL-L2300D/HL-L2340DW) LWAd = 6.46 B (A) (HL-L2360DN/HL-L2365DW) LWAd = 6.66 B (A)
Ready *1*2 | LWAd = 4.55 B (A)
Printing (Quiet Mode) | LWAd = 6.06 B (A)
Temperature | Operating | 10 to 32 °C
Storage | 0 to 40 °C
Humidity | Operating | 20 to 80% (without condensation)
Storage | 10 to 90% (without condensation)

*1
Measured in accordance with the method described in RAL-UZ171.
*2
Office equipment with LWAd>6.30 B(A) is not suitable for use in room where people require high levels of concentration. Such equipment should be placed in separate rooms because of noise emissions.

Related Information
  - Specifications
  - Settings Table
  - WLAN Enable (Wireless Network Only)

Go to top of page