Home > Network > Advanced Network Features > Print the Network Configuration Report

### Print the Network Configuration Report

Related Models:HL‑L2340DW / HL‑L2360DN / HL‑L2365DW
The Network Configuration Report lists the current network configuration, including the network print server settings.

- Node Name: The Node Name appears on the current Network Configuration Report. The default Node Name is "BRNxxxxxxxxxxxx" for a wired network or "BRWxxxxxxxxxxxx" for a wireless network (where "xxxxxxxxxxxx" is your machine's MAC Address / Ethernet Address.)
- If the IP Address on the Network Configuration Report shows 0.0.0.0, wait for one minute and try printing it again.
- You can find your machine's settings, such as IP address, subnet mask, node name, and MAC Address on the report, for example:
  - IP address: 192.168.0.5
  - Subnet mask: 255.255.255.0
  - Node name: BRN000ca0000499
  - MAC Address: 00-0c-a0-00-04-99

1. Press or to select the Machine Info. option, and then press OK.
2. Press or to select Print NetSetting.
3. Press OK.

Related Information
  - Advanced Network Features
  - Where Can I Find My Brother Machine's Network Settings?
  - Use the Network Connection Repair Tool (Windows®)
  - My Brother Machine is Not Found on the Network During Printer Driver Installation.
  - I Want to Check that My Network Devices are Working Correctly.
  - Access Web Based Management
  - Locate Network Settings When Using Web Based Management
  - Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)
  - Locate Network Settings When Using BRAdmin Professional 3 (Windows®)

Go to top of page